Positions quoted in this Preliminary Notice reproduced below are referred to WGS84 or a compatible datum and may be plotted directly on this ENC. 												Some or all of the information contained in this Notice to Mariners may have been included on the ENCs affected.																			
4940(P)/25 DENMARK —  Islands — Works. Buoyage. Depths. Coastline.																			
Source: Danish Notice 18/317(P)/25 and ENC DK5RONNE																			
																			
	1.	*Significant changes to depths, aids to navigation and coastline are taking place within the port of Ronne.																	
																			
	2.	Works are taking place to remove the mole in the following positions:																	
																			
		55° 05' .797N. , 14° 41' .316E.																	
		55° 05' .830N. , 14° 41' .228E.																	
																			
	3.	Buoys have been established to mark the works in the following positions:																	
																			
		Characteristic				Buoy Type						Position				
		Unlit					yellow spar buoy, with cross topmark			55° 05' .794N. , 14° 41' .275E.				
		Fl(3)Y.10s				yellow can buoy, with cross topmark			55° 05' .800N. , 14° 41' .336E.				
		Unlit					yellow spar buoy, with cross topmark			55° 05' .813N. , 14° 41' .324E.				
																			
	4.	The port hand light-buoy, Q.R, in position 55° 05' .748N. , 14° 41' .111E. has moved to position 55° 05' .786N. , 14° 41' .304E.																	
																			
	5.	*Mariners are advised to navigate with caution in the area and consult the local port authority for the latest information.																	
																			
	6.	*The chart will be updated when works are complete.																	
																			
		(WGS84 DATUM)