Positions quoted in this Preliminary Notice reproduced below are referred to WGS84 or a compatible datum and may be plotted directly on this ENC. 									
Some or all of the information contained in this Notice to Mariners may have been included on the ENCs affected.																		
5667(P)/25 DENMARK —  Islands — Works. Buoyage. Depths. Coastline. Light. Restricted area.															
Source: Danish Notices 42/853/25, 44/898/25, 46/929/25, 47/954/25, 47/961/25, 48/985/25 and ENC DK5RONNE																																		
	1.	Significant changes to depths, aids to navigation and coastline are taking place within the port of Rønne.																															
	2.	*An entry prohibited limit marked by seven unlit spar buoys, seven lit spar buoys, Fl(3)Y.30s and a starboard hand spar buoy, Q.G have all been deleted, along the following bounded positions:																											
		55° 05' .487N. , 14° 40' .693E.	
															
		55° 05' .532N. , 14° 40' .786E.	
															
		55° 05' .559N. , 14° 40' .778E.	
															
		55° 05' .681N. , 14° 40' .581E.
																
		55° 05' .674N. , 14° 40' .493E.	
															
		55° 05' .645N. , 14° 40' .439E.																
																		
	3.	*The extension of the outer mole has been completed joining the following positions:																													
		55° 05' .526N. , 14° 40' .758E.	
															
		55° 05' .659N. , 14° 40' .545E.																
																		
	4.	*A light, Fl(1+4)G.5s has been established in position 55° 05' .653N. , 14° 40' .556E.																													
	5.	*Work has now been completed, and moles have been removed in the following positions:																													
		55° 05' .797N. , 14° 41' .316E.	
															
		55° 05' .830N. , 14° 41' .228E.																
																		
		and																
																		
		*55° 05' .670N. , 14° 41' .237E.
																
		*55° 05' .702N. , 14° 41' .188E.																
																		
	6.	*Several lit and unlit buoys have been deleted in the following positions:																
																		
		Characteristic					Buoy Type							Position
			
		Fl(3)Y.10s					spar buoy, with x-shape topmark					55° 05' .544N. , 14° 41' .048E.	
		
		Unlit						spar buoy, with x-shape topmark					55° 05' .538N. , 14° 41' .090E.	
		
		Unlit						spar buoy, with x-shape topmark					55° 05' .531N. , 14° 41' .130E.	
		
		Fl.R.5s						spar buoy, with cylinder topmark				55° 05' .516N. , 14° 41' .217E.	
		
		Q.G						spar buoy, with cone point up topmark				55° 05' .694N. , 14° 41' .163E.	
		
		Fl(3)Y.10s					spar buoy, with x-shape topmark					55° 05' .711N. , 14° 41' .200E.	
		
		Q.R						can buoy							55° 05' .750N. , 14° 41' .110E.			
																		
	7.	*Mariners are advised to navigate with caution in the area as extensive changes have taken place and consult the local port authority for the latest information.																												
	8.	*The chart will be updated when full details are known.																
																		
	9.	*Former Notices 3200(P)/25 and 4940(P)/25 are cancelled.																
																		
		(WGS84 DATUM)