INTRACOASTAL WATERWAY
Project Depths:
3.6 meters/12 feet Norfolk, VA to Fort Pierce, FL via Route 1.
2.1 meters/9 feet Norfolk to Albemarle Sound, via Route 2,
Great Dismal Swamp Canal.
3.0 meters/10 feet Fort Pierce, FL to Miami, FL.
2.1 meters/7 feet Miami, FL to Cross Bank, Florida Bay.
Consult the U.S. Army Corps of Engineers for controlling depths and U.S. Coast Guard Local Notice to Mariners for other navigation hazards or restrictions.
Uncharted shoals may exist in areas which have not been recently surveyed. Please report shoals and obstructions at: https://www.nauticalcharts.noaa.gov/customer-service/assist/
Distances:
Mariners are advised to follow the aids to navigation and avoid charted shoals and obstructions.