OVERHEAD CROSSINGS
Overhead crossings between Plymouth and Palmyra Landing: 
Power Cables, minimum AUTH CL 22.8 Meters / 75 Feet (Normal Water Level).  
Bridges, minimum HOR CL 22.8 Meters / 75 Feet, minimum VERT CL 1.2 Meters / 4 Feet (HW).