SYDNEY HARBOUR BRIDGE
The maximum clearance height is 51.3m at the centre, while
for the northern lead it is not less than 50.5m and for the
southern lead not less than 48.6m. When in use, a travelling
gantry, marked at night by yellow lights, decreases the above
clearances by 3.2 metres.
